Xyyzz

Low Pt Anodes for Polymer Electrolyte Fuel Cells

Jack Left (1), Mike Middle (1,2), Peter Wright (2)

(1) Fuel Cells Forever, Inc., Clean Town/ New Wonderland;

(2) Faculty of Sciences and Technology, New Town/Wonderland;

Tel.: +41-56-987-1234, Mobile: +41-22-333-444

[jsample@fastmail.com](mailto:jsample@fastmail.com)

Abstract

This is a sample text: The reduction of the Pt catalyst loading in Polymer Electrolyte Fuel Cells (PEFC) is a premise for a commercial introduction of fuel cell electric cars. In the state of the art, the Pt loading for the anode varies between 30 and 100 µgr/sqcm. In this work, low platinum loadings in the range of 2 to 25 µgr/sqcm were sputtered onto carbon cloth substrates that were used as PEFC anodes. Membrane electrode assemblies were prepared by hot pressing with Nafion 212 and commercial cathodes. We succeeded in reducing the Pt loading of PEFC down to 25 µgr/sqcm without significant loss of fuel cell performance compared to commercial electrodes 500 µgr/sqcm. Longevity tests at constant current densities showed nearby stable voltages for at least 1’000 hrs. ………

**Instructions:**

* Please use the formatted template below.
* Abstracts must not be longer than 1 page (a graphic or picture is welcome).
* **Rename the file**: MEEP2023\_Short-title\_Family-name\_Given-name\_Current-Version.docx   
  (Number "\_01" is for first submitted version, "\_02" for the second, etc.)
* **Overwrite the Sample Text** with your content, but keep the formatsas given.
* Numbering: Do not write "(1)" in the header, if there is only one institution.
* **Delete all red and yellow comments**. Xyyzz must be left untouched.
* Upload you one-page Abstract by 23 January 2023 at the latest.   
  [www.i-MEEP.com/upload](http://www.i-MEEP.com/upload)   
  Indicate your presentation preference: Oral or Poster.

**Special Issue:** We are currently investigating the feasibility of a peer reviewed Special Issue specifically for MEEP contributions. If you would be interested in being considered, please select this option at the time of upload. It is always possible to change your mind at a later date.

Xyyzz

Low Pt Anodes for Polymer Electrolyte Fuel Cells

**Template**

with **only one institution**

no (1) etc. required

Jack Left, Mike Middle, Peter Wright

Fuel Cells Forever, Inc., Clean Town/Wonderland

Tel.: +41-56-987-1234, Mobile: +41-22-333-444

[jsample@fastmail.com](mailto:jsample@fastmail.com)

Abstract

This is a sample text: The reduction of the Pt catalyst loading in Polymer Electrolyte Fuel Cells (PEFC) is a premise for a commercial introduction of fuel cell electric cars. In the state of the art, the Pt loading for the anode varies between 30 and 100 µgr/sqcm. In this work, low platinum loadings in the range of 2 to 25 µgr/sqcm were sputtered onto carbon cloth substrates that were used as PEFC anodes. Membrane electrode assemblies were prepared by hot pressing with Nafion 212 and commercial cathodes. We succeeded in reducing the Pt loading of PEFC down to 25 µgr/sqcm without significant loss of fuel cell performance compared to commercial electrodes 500 µgr/sqcm. Longevity tests at constant current densities showed nearby stable voltages for at least 1’000 hrs. ………